BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2111
Alerting timeout for cordless

This command is used to set the system parameter ALERTING TIMEOUT. Alerting timeout is used by ICCU2 firmware as limit how long it waits for alerting signal from cordless software.

After receiving timeout diversion on not available is executed.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004