BusinessPhone Communication Platform 6.0
Commands > Commands 6000...6999

## 6802
Tenant password

This command can be used to define a password of 1 to 16 digits for a given tenant group which allows access to a specific tenant group when doing call metering activities. Tenant groups are needed, if several customers want to share one ASB150. They can separate their extensions and trunks into a maximum of 16 tenants.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004