BusinessPhone Communication Platform 6.0
Facility Description – General

## ASB150 02 Licensing

### ASB 150 02 Release 9 - Release 13 Licensing

Together with the introduction of the ASB 150 02 Release 9, a hardware key based licensing concept was introduced.

Most of the features, that were introduced from the Software Release ASB 150 02 Release 9 and upwards can only be enabled by a FECU (Feature Enabling Circuit Unit), which is connected to the CPU‑D4.
Each major commercial release (e.g. BusinessPhone Version 3, Version 4, Version 5 ...) has its own FECU series, covering several packages.

#### BusinessPhone Communication Platform - Version 3 (ASB 150 02 R9 / R10)

FECU article number: KDUBS 130 06 / x
(x = Package 1-10)

Package 1: |  | Basic Functions R9 / R10

Package 2: |  | Standard digital networking with max. 32 trunk interfaces

Package 3: |  | Standard digital networking with unlimited trunk interfaces

Package 4: |  | Full digital networking with max. 32 trunk interfaces

Package 5: |  | Full digital networking with unlimited trunk interfaces

Package 6: |  | CTI

Package 7: |  | CTI+ Standard digital networking with max. 32 trunk interfaces

Package 8: |  | CTI + Standard digital networking with unlimited trunk interfaces

Package 9: |  | CTI + Full digital networking with max. 32 trunk interfaces

Package 10: |  | CTI + Full digital networking with unlimited trunk interfaces

#### BusinessPhone Communication Platform - Version 4 (ASB 150 02 R11)

FECU article number: KDUBS 130 07 / x
(x = Package 1-10)

Package 1: |  | Basic Functions R11

Package 2: |  | Standard digital networking with 32 trunk interfaces

Package 3: |  | Standard digital networking with unlimited trunk interfaces

Package 4: |  | Full digital networking with 32 trunk interfaces

Package 5: |  | Full digital networking with unlimited trunk interfaces

Package 6: |  | CTI + Full digital networking with 4 trunk interfaces

Package 7: |  | CTI + Standard digital networking with 32 trunk interfaces

Package 8: |  | CTI + Standard digital networking with unlimited trunk interfaces

Package 9: |  | CTI + Full digital networking with 32 trunk interfaces

Package 10: |  | CTI + Full digital networking with unlimited trunk interfaces

#### BusinessPhone Communication Platform - Version 5.0 (ASB 150 02 R12)

FECU article number: KDUBS 130 12 / x
(x = Package 1-10)

Package 1: |  | Basic Functions R12+ Full digital networking with 2 trunk interfaces

Package 2: |  | Standard digital networking with 32 trunk interfaces

Package 3: |  | Standard digital networking with unlimited trunk interfaces

Package 4: |  | Full digital networking with 32 trunk interfaces

Package 5: |  | Full digital networking with unlimited trunk interfaces

Package 6: |  | CTI + Full digital networking with 4 trunk interfaces

Package 7: |  | CTI + Standard digital networking with 32 trunk interfaces

Package 8: |  | CTI + Standard digital networking with unlimited trunk interfaces

Package 9: |  | CTI + Full digital networking with 32 trunk interfaces

Package 10: |  | CTI + Full digital networking with unlimited trunk interfaces

#### BusinessPhone Communication Platform - Version 5.1 (ASB 150 02 R13)

FECU article number: KDUBS 130 13 / x
(x = Package 1-10)

Package 1: |  | Basic Functions R13+ Full digital networking with 2 trunk interfaces

Package 2: |  | Standard digital networking with 32 trunk interfaces

Package 3: |  | Standard digital networking with unlimited trunk interfaces

Package 4: |  | Full digital networking with 32 trunk interfaces

Package 5: |  | Full digital networking with unlimited trunk interfaces

Package 6: |  | CTI + Full digital networking with 4 trunk interfaces

Package 7: |  | CTI + Standard digital networking with 32 trunk interfaces

Package 8: |  | CTI + Standard digital networking with unlimited trunk interfaces

Package 9: |  | CTI + Full digital networking with 32 trunk interfaces

Package 10: |  | CTI + Full digital networking with unlimited trunk interfaces

The term “trunk interface” in the table above, has the meaning of one (1) connection used for private network communication. It correspondsence to one (1) B-channel of the BA or PRA or (1) voice channel on the , which is used for private network traffic.

Features which were introduced in a Release earlier than ASB 150 02 R9 are always enabled, and therefore also accessible if no FECU is connected to the CPU-D4/CPU-D5. Furthermore fault corrections to existing unprotected features, as well as small feature improvements are always enabled.
Only two features are excluded from this philosophy: These are the "BusinessLink for Novell" and "proprietary CTI Interface", which were introduced in ASB 150 02 R8. To run the "BusinessLink for Novell" and "proprietary CTI Interface" on the system with R9 Software or upwards, the related FECU (see following table) is required.

The Package 1 always represents the new basic functionality of the Release, which is of course also included in all packages with a higher index.
If you upgrade a system to a higher SW-Release, without changing the FECU although the new Release has its own FECU series (separate article number), the system will remain on the same feature level, except for those features that are not protected.

#### Functionality enabled in ASB 150 02 depending on the connected FECU

- KDUBS 130 06 / 1-10 (ASB 150 02 R9, R10)
- KDUBS 130 07 / 1-10 (ASB 150 02 R11)
- KDUBS 130 12 / 1-10 (ASB 150 02 R12)
- KDUBS 130 13 / 1-10 (ASB 150 02 R13)

The entries in the table are indicating the minimum FECU version (last two digits of the article code), for the respective feature. The FECU version may not specifically be equal to the SW version the feature was introduced.

Feature | FECU KDUBS 130 xx/1 | FECU KDUBS 130 xx/2 | FECU KDUBS 130 xx/3 | FECU KDUBS 130 xx/4 | FECU KDUBS 130xx/5 | FECU KDUBS 130 xx/6 | FECU KDUBS 130 xx/7 | FECU KDUBS 130 xx/8 | FECU KDUBS 130 xx/9 | FECU KDUBS 130 xx/10 | FECU KDUBS 130 xx/11
Account numbers (verified) | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 |
ACD - Multiple call codes | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 |
ACD - Queue Exit | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 |
Automatic Redial | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 |
Call metering - Multiple tariff handling | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 |
Clock and diary (synchronisation with ISDN) | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 |
Conversation recording | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 |
CTI - proprietary CTI Interface * |  |  |  |  |  | 06 | 06 | 06 | 06 | 06 |
CTI - BusinessLink for Novell * |  |  |  |  |  | 06 | 06 | 06 | 06 | 06 |
CTI - BusinessLink for Windows NT |  |  |  |  |  | 06 | 06 | 06 | 06 | 06 |
CTI - BusinessLink for Win NT - only Support of OWS, AAO (2 users) | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 |
CTI Groups 9-16 |  |  |  |  |  | 07 | 07 | 07 | 07 | 07 |
CTI - Enhanced CIL function |  |  |  |  |  | 06 | 06 | 06 | 06 | 06 |
Fax Extension | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 |
Fictive number - Direct diversion | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 |
Fictive number >16 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 |
Fictive number - CTI monitoring | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 |
Group hunting (PBX-Group) with parallel distribution | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 |
Individual external diversion | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 |
Individual number translation external | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 |
Individual number translation internal | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 |
Information via keypad | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 |
Integrated Cordless - GAP 1.0 protocol | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 |
Integrated Cordless - GAP 2.0 protocol | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 |
IP Extension | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 |
ISDN Caller List | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 |
ISDN Call forwarding with partial rerouting | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 |
ISDN - CLIR override | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 |
ISDN - BA in a point to multiPoint configuration | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 |
Mailbox-system - personal greeting | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 |
Mailbox-system - outcall notification | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 |
Music on hold- integrated (1 source) | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 |
Music on hold (1 integrated and 12 external sources or 13 external sources) | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 |
National specific functions - Croatia: Adaptation of CN numbering plan | 12 | 06 | 06 | 06 | 06 | 07 |  |  | 06 | 06 |
National specific functions - Spain: Ibercom Indicator | 12 | 06 | 06 | 06 | 06 | 07 | 06 | 06 | 06 | 06 |
National specific functions - Austria: Support of packet mode terminals | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 | 07 |
National specific functions - Italy: ISDN three party conference | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 |
National specific functions - New Zealand: Centrex hook flash over ISDN | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 |
Networking - based on digital/VoIP lines with QSIG (32 trunk interfaces) |  | 06 | 06 | 06 | 06 |  | 06 | 06 | 06 | 06 |
Networking - based on digital/VoIP lines with QSIG (unlimited trunk interfaces) |  |  | 06 |  | 06 |  |  | 06 |  | 06 |
Networking - based on digital/VoIP lines with QSIG+UUS (2 trunk interfaces) | 12 |  |  | 06 | 06 | 07 |  |  | 06 | 06 |
Networking - based on digital/VoIP lines with QSIG+UUS (4 trunk interfaces) |  |  |  | 06 | 06 | 07 |  |  | 06 | 06 |
Networking - based on digital/VoIP lines with QSIG+UUS (32 trunk interfaces) |  |  |  | 06 | 06 |  |  |  | 06 | 06 |
Networking - based on digital/VoIP lines with QSIG+UUS (unlimited trunk interfaces) |  |  |  |  | 06 |  |  |  |  | 06 |
Networking - based on digital/VoIP lines with UUS mapped into GFP | 12 |  |  | 07 | 07 | 07 |  |  | 07 | 07 |
Networking - based on digital/VoIP lines -Central. Operator #) | 12 |  |  | 07 | 07 | 07 |  |  | 07 | 07 |
O&M - Swapping boards during operation | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 |
O&M -Remote SW upgrading | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 |
O&M -Remote FW upgrading | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 | 12 |
O&M -Remote D4 FW upgrading | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 | 06 |
Voice Outcall Notification | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 | 13 |
VoIP Gateway |  |  |  |  |  |  |  |  |  |  | 13

X * |  | Feature was introduced in a Release earlier than ASB 150 02 R9 The "proprietary CTI Interface" and "BusinessLink for Novell" were already released in ASB 150 02 R8 and are always enabled on the CPU-D3. In conjunction with the CPU-D4/CPU-D5 a FECU device is required. |
#) |  | Following features are covered by the name COP - Supervision of busy with recall at free (similar to the Call Back on busy function) - Camp on - Intrusion with forced release - Recall at No Answer |

Together with ASB 150 02 Release 14 the software licensing concept based on the hardware key FECU is replaced by a software key concept.

### ASB150 02 Release 14 (or higher) Licensing

Together with ASB 150 02 Release 14 the software licensing concept based on the hardware key FECU is replaced by a software key concept.

The software key is represented by a license file which is stored on the CPU‑D5 if available. If there is no CPU-D5 in the system (upgraded system based on a CPU-D4) it is possible to store the license file on the compact flash card of the MFU, IPU or VMU-HD.

Equal to the former FECU Index 1, there exists a basic license entry in the license file, which covers all basic features up to the latest release. On top of the basic license entry there exists additional license entries for following features:

- Mobile Extension
- Unified Messaging
- CTI
- Networking
- VoIP Gateway

Note

The Unified Messaging license requires in addition also a CTI license.
(£ 20 Unified Messaging users 5 CTI users are required, >20 Unified Messaging users, 80 CTI users are required)

The licensed features are available in different modularity steps. From commercial point of view, these modularity steps are defined as so called color packs which are available in yellow, orange and red color.

The entries in the table are indicating the minimum article number for the respective feature.

Feature | Basic License | Mobile Extension FALBS 102 44 /_ | Networking FALBS 102 49/Y | Networking FALBS 102 49/O | Networking FALBS 102 49/R | CTI FALBS 102 46/Y FALBS 102 46/O | Unified Messaging FALBS 102 45/_ | VoIP Gateway FALBS 102 50/Y
Account numbers (verified) | X |  |  |  |  |  |  |
ACD - Multiple call codes | X |  |  |  |  |  |  |
ACD - Queue Exit | X |  |  |  |  |  |  |
Automatic Redial | X |  |  |  |  |  |  |
BackStage 5.0 (or higher) 2 Reference users without the need of a WIBU-Box and a CTI License | X |  |  |  |  |  |  |
Call metering - Multiple tariff handling | X |  |  |  |  |  |  |
Clock and diary (synchronisation with ISDN) |  |  |  |  |  |  |  |
Conversation recording | X |  |  |  |  |  |  |
CTI - proprietary CTI Interface |  |  |  |  |  | X |  |
CTI - BusinessLink for Novell * |  |  |  |  |  | X |  |
CTI - BusinessLink for Windows NT |  |  |  |  |  | X |  |
CTI - BusinessLink for Win NT - only Support of OWS, AAO, BackStage 5.0 (2 users). | X |  |  |  |  |  |  |
CTI Groups 9-16 |  |  |  |  |  | X |  |
CTI - Enhanced CIL function |  |  |  |  |  | X |  |
Fax Extension | X |  |  |  |  |  |  |
Fictive number - Direct diversion | X |  |  |  |  |  |  |
Fictive number >16 | X |  |  |  |  |  |  |
Fictive number - CTI Monitoring | X |  |  |  |  |  |  |
Group hunting (PBX-Group) with parallel distribution | X |  |  |  |  |  |  |
Individual external diversion | X |  |  |  |  |  |  |
Individual number translation external | X |  |  |  |  |  |  |
Individual number translation internal | X |  |  |  |  |  |  |
Information via keypad | X |  |  |  |  |  |  |
Integrated Cordless - GAP protocol | X |  |  |  |  |  |  |
IP Extension | X |  |  |  |  |  |  |
ISDN Caller List | X |  |  |  |  |  |  |
ISDN Call forwarding with partial rerouting | X |  |  |  |  |  |  |
ISDN - CLIR override | X |  |  |  |  |  |  |
ISDN - BA in a point to multiPoint configuration | X |  |  |  |  |  |  |
Mailbox-system - personal greeting | X |  |  |  |  |  |  |
Mailbox-system - outcall notification | X |  |  |  |  |  |  |
Mobile Extension |  | X |  |  |  |  |  |
Music on hold- integrated (1 source) | X |  |  |  |  |  |  |
Music on hold (1 integrated and 12 external sources or 13 external sources). | X |  |  |  |  |  |  |
National specific functions - Brazil: Collect Call Blocking | X |  |  |  |  |  |  |
National specific functions - Spain: Ibercom Indicator | X |  | X | X | X |  |  |
National specific functions - Croatia: Adaptation of CN numbering plan | X |  | X | X | X |  |  |
National specific functions - Austria: Support of packet mode terminals | X |  |  |  |  |  |  |
National specific functions - Italy: ISDN three party conference | X |  |  |  |  |  |  |
National specific functions - New Zealand: Centrex hook flash over ISDN | X |  |  |  |  |  |  |
Networking - based on digital/VoIP lines with QSIG (unlimited trunk interfaces) |  |  | X |  |  |  |  |
Networking - based on digital/VoIP lines with QSIG+UUS (2 trunk interfaces) | X |  |  |  |  |  |  |
Networking - based on digital/VoIP lines with QSIG+UUS (32 trunk interfaces) |  |  |  | X |  |  |  |
Networking - based on digital/VoIP lines with QSIG+UUS (unlimited trunk interfaces) |  |  |  |  | X |  |  |
Networking - based on digital/VoIP lines with UUS mapped into GFP | X |  |  | X | X |  |  |
Networking - based on digital/VoIP lines - Central. Operator #) | X |  |  | X | X |  |  |
O&M - Swapping boards during operation | X |  |  |  |  |  |  |
O&M -Remote SW upgrading | X |  |  |  |  |  |  |
O&M -Remote FW upgrading | X |  |  |  |  |  |  |
O&M -Remote D4 FW upgrading | X |  |  |  |  |  |  |
O&M - Cordless remote programming | X |  |  |  |  |  |  |
Unified Messaging |  |  |  |  |  |  | X |
VoIP Gateway |  |  |  |  |  |  |  | X

* |  | The "proprietary CTI Interface" and "BusinessLink for Novell" were already released in ASB 150 02 R8 and are always enabled on the CPU-D3. In conjunction with Release 14 or higher a CTI license is required. |
#) |  | Following features are covered by the name COP - Supervision of busy with recall at free (similar to the Call Back on busy function) - Camp on - Intrusion with forced release - Recall at No Answer |

Revision: C © Ericsson Enterprise 2004