BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2644
Okay, continue tone

The tone is used to give the user a confirmation that something expected has occurred, e. g. that a recorded message is played to the calling party and that the calling party will be connected in speech mode.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004