BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2145
GW RAS transport address

Defines a list of 35 RAS transport addresses of trusted GWs which are accepted by the GK to register with it.

##### Valid data

|  | Network IP address |  | Port number |
1-35 |  | 0.0.0.0 - 255.255.255.255 |  | 0-65535 |
1-35 |  | 0.0.0.0 (default) |  | 0 (default) |

Note

If the Port number is 0, then the Gatekeeper does not check the port number of the trusted Gateway

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004