BusinessPhone Communication Platform 6.0
Commands > Commands 7000...7999

## 7801
RSU-group reservation

With this command it is possible to reserve each RSU-group (Register Signalling Unit) for one register signalling application. The 2 different applications are traffic register signalling and voice services. If none of these is specified, both will be handled.

Values:

0 = No RSU-groups reserved (default) |  |

1 = Reserved for traffic register signalling |  |

2 = Reserved for voice services |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004