BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2236
Own country code

This command defines the own country code. It is used to prefix a calling/connected number, which is part of the number plan E.164 before it is sent to the private network.

Note

Only relevant for proprietary networks

##### Valid data

empty |  | (default) |
1-4 digits |  | do not include predigits, such as 00 |

Example:

An incoming call to the private network will be terminated in a node, which is located in another country. In the PNR table of the gateway node the TON for the desired node is defined as INTERNATIONAL. Due the fact that the received calling line number is of TON “NATIONAL” it has to be modified to a correct international number before it can be sent to the private network. Modification is done by adding the country code of the gateway exchange

Calling number |  | 76825047 (NAT) |
Country code (command 2236) |  | 43 |
TON public calling (command 9105) |  | INTERNATIONAL |

In this case, the calling number being sent to the private network will be 4376825047.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004