BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1912
Termination in ASB 150

The command is used to define the network termination for the current ISDN-link. It specifies the operation mode for layer 1, 2 and 3 as well as the link synchronisation and the actions in case of call collision and error conditions. There are four choices:

Termination Remote: |  | Synchronisation: |
USER public slave |  | NETWORK L1 master private master |
USER private slave |  | NETWORK L1 slave private slave |

Public network: The link shall always be defined as “User in public network”.

Private network: If the opposite side is configured as network then the link shall be defined as “user in private network”. If the opposite side is configured as user then the link shall be defined as “Network-layer 1 sync master”, but, if the link is connected to a router (or other equipment) that are layer 2 and layer 3 transparent but layer 1 sync master, then the link may be set as “Network-layer 1 sync slave”.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004