BusinessPhone Communication Platform 6.0
Commands > Commands 9000...9999

## 9110
1st-route choice

The directory number for the 1-st route choice is defined with command 9110.

Alternative routing.

When all trunks in the 1-st route are busy, the call can be sent via another route. An alternative route shall be defined for the call to be rerouted.

Three different alternative routes can be defined.

The 2-nd is defined with command 9120 2nd-route choice.

The 3-rd is defined with command 9130 3-rd route choice.

The 4-th is defined with command 9140 4-th route choice.

The route directory number must exist before the command 91.. is programmed.

##### Valid data

0 - 4 |  | digits |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004