BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0xA8
E2-Write Sequence Error

Default definition: |  | ERROR |
Used by block: |  | SP |
Category: |  | DESIGNER |

The serial communication processor (SP) on the CPU board has detected an error in the E2-write sequence.

- D1:
- D2: Type of error

- 01h: CP has written (indicated write complete (NMI)) without enabling E2-memory first.
- 02h: CP has requested enabling of E2-write before earlier write was ready.
- 03h: CP has requested enabling of E2 write, but no writing was done within 100 ms.

- D3: Undefined
- D4: Undefined

Revision: I © Ericsson Enterprise 2004