BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0145
Relay control

This command specifies how the relay on the I/O-board in the telephone instruments, type DBC 2xx, will be directed.

##### Valid data

No functions |  | (default) |
Follows bell |  |  |
Follows buys state of intrument |  |  |
Follow message LED |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004