BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1017
Reroute on incomplete number?

The command is used for direct in-dialing and private trunks for rerouting incoming calls to the rerouting position, if an inadequate number of digits has been received from a superior exchange. For rerouting to take place it is necessary that the rerouting position has been programmed, see commands 1103 Reroute position at day and 1104 Reroute position at night.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004