BusinessPhone Communication Platform 6.0
Commands > Commands 6000...6999

## 6302
Log duration time

This command can be utilised if it is desired to log outgoing external calls (see command 6301 Log outgoing calls ?), but exclude “short” calls.

The command is used to set a minimum call duration time for an outgoing external call to be logged.

Further prerequisites can be defined for determining which outgoing external calls shall be logged, see commands 6303 Log minimum meter pulses and 6306 Log dialled numbers beginning with 0-6315 Log dialled numbers beginning with 9.

With the minimum call duration time = 0000, outgoing external calls will be logged irrespective of call

##### Valid data

0-59min 0-59secs |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004