BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0xB0
E2PROM Fatal Error (Stop 1)

Default definition: |  | STOP + NOPROG |
Used by block: |  | E2 |
Category: |  | MAINTENANCE |

This code will always cause a system restart that cannot be reprogrammed. The yellow led on the CPU front will indicate the stop reason with a single-flash led cadence. The warning code is used by the E2-handler, when an error concerning the first EEPROM-chip is detected during the initiation phase. This chip contains, among other data, a configuration variable, indicating, which EEPROM-chips that are mounted on the CPU board. This variable must be accessible during the initiation of the E2-handler.

- D1:
- D2: Type of error

- 01h: The first EEPROM chip (position 190) is not mounted or contains illegal data.
- 02h: An error has been detected, when a new value of the configuration variable should be updated at the end of the E2-handler initiation.

- D3: Undefined
- D4: Undefined

Revision: I © Ericsson Enterprise 2004