BusinessPhone Communication Platform 6.0
Commands > Commands 4000...4999

## 4305
Voice message quality

Voice messages, voice information and voice answers (recorded announcements) are stored on “voice memory boards”, VMUs.

The storage capacity, in seconds, of the board can be increased at the expense of speech (voice) quality.

Via commands 4305 Voice message quality-4307 Voice answer quality it is possible to determine the speech quality desired for voice messages, voice information and voice answers.

This command determines the quality is to be used for voice messages (high quality or not).

Yes |  | (high quality)

No |  | (normal quality)

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004