BusinessPhone Communication Platform 6.0
Commands > Commands 4000...4999

## 4501
Predefined info - Text

Via this command the text string for predefined information is stated. The text string can comprise a maximum of 35 characters.

Note

The first 20 characters will be displayed in the top row and the last 13 in the second row of the telephone display.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004