BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1942
UU-information length for UUS service 1

This command states which maximal UUI (User-to-User Information) length in UUS (User-toUser Signalling) service 1 is supported at this interface.

##### Valid data

0 |  | 128 octets |
1 |  | 32 octets |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004