BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x48
Manual Logging

Default definition: |  | UNDEFINED |
Used by block: |  | ALL |
Category: |  | DESIGNER |

This code is used, when a warning is caused intentionally by some manual user action in order to create a tracelog, etc.

- D1: Directory number of own party, high byte
- D2: Directory number of own party, low byte
- D3: Directory number of connected party, high byte
- D4: Directory number of connected party, low byte

Revision: I © Ericsson Enterprise 2004