BusinessPhone Communication Platform 6.0
Dialogs

## Trunk Route - Copy Parameters

You can copy the settings of an existing trunk route to a new route.

### To copy the settings:

- In the Configuration directory tree on the left side, open the “Trunks” menu and click on “Trunk Routes” to open the Trunk Routes dialog.
- Click on the Parameters button of a trunk. This will open the Trunk Route Parameters dialog.
- Select the facilities that should get the current route parameters. There are two ways to select a group:

- Mark the check box “(Un)Select commands”. If the box is checked, all parameters listed below are selected automatically. To deselect all parameters, just click again in the check box to remove the tick.
- Enter the directory name and number in the appropriate fields and click on the Select button.

- Click on the Copy button. The parameter settings are copied to the selected routes.

#### Actions

Select |  | To select the entered directory range. |
Submit |  | To copy the current parameter settings to all selected trunk routes. |
Close |  | To close the window and abort the parameter settings copy. |

Revision: B © Ericsson Enterprise 2004