BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2093
Conversation recording tone

This command defines if the system is permitted to generated a conversation tone during recording of an established call in speech.

##### Valid data

Yes |  | (default) |
No |  |  |

Default data: No

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004