BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8103
Mode digit

This command is used to determine the use of the mode digit. The following alternatives are possible:

0 = the mode digit is not used |  |

1 = the mode digit is used and is placed before the paging code |  |

2 = the mode digit is used and is placed after the paging code |  |

The mode digit specifies the type of paging, e.g. display paging, voice paging, etc. The position of the mode digit depends on the method used by the paging equipment for receiving mode digits.

A paging code, i. e. the identity of the paging receiver, can also be sent to the paging equipment without mode digit.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004