BusinessPhone Communication Platform 6.0
Facilities

## Last External Number Redial

## Definition

ASB 150 02 automatically stores the external number dialled last (including ROUTE ACCESS CODE). The user may repeatedly send the directory number.

(Similar facility: Saved external number redial.)

## Use

External directory numbers may easily be repeated, especially if the called extension is busy or does not answer.

## Operation

### Storing of external numbers

Each dialled external number will automatically be stored, irrespective of how it was dialled - manually, using ABBREVIATED NUMBERS or with a NAME-SELECTION KEY.

The new directory number replaces the previous one.

If you want to delete the stored number, you only have to select the route access code. In this case the last number redial contains only the route access code - the number dialled previously is erased.

#### Redialling of the last external number

1. Press three times the key * (s* * *) to redial the external number.

The access code for LAST NUMBER REDIAL may also be stored in a NAME-SELECTION KEY.

## Capacity

The last number redial stores the TRUNK ACCESS CODE or the ROUTE ACCESS CODE together with the dialled external number.

ASB 150 02 stores up to 24 digits. In case that more than 24 digits have been dialled, the last number redial contains the first 24 digits.

## Limitations

Initialization of the system clears the last number redial.

## Programming

None

## Equipment

No additional hardware necessary.

Revision: C © Ericsson Enterprise 2004