BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8101
Number of paging digits

For each paging call a paging code is sent to the paging equipment. The paging code determines which paging receiver(s) shall receive the call.

The number of digits in the paging code depends on the method used by the paging equipment for receiving paging codes. This is often programmable in the paging equipment.

This command is used to determine the number of digits in the paging code to the paging equipment. Range of values: 1-4 digits.

For each paging receiver a paging code can be defined with command 8202 Search code. If the paging equipment requires more digits than the stated paging code, initial zeroes are added. If, on the other hand, the paging equipment cannot accept all digits in the stated paging code, the final digits in the paging code will be discarded.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004