BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2275
Automatic Redial Table

This command defines the number of redial attempts and the time intervals (in second between the attempts) when automatic redial calls are performed. A maximum of 10 entries are possible.

Note

Vacant entries are set to ZERO (0).

##### Valid data

Valid values: |  | 15 - 255 sec. (per entry) |
empty entry: |  | 0 (show blanks to user) |
Initial values (default): |  | 30 (1st. attempt) |
|  | 60 (2nd. attempt) |
|  | 60 (3rd. attempt) |
|  | 0 (for 7 left attempts) |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004