BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2023
External voice mail directory number

An external voice mail system can be connected to ASB 150 via an analogue extension board.

A programmable key can be defined for the external voice mail function. The LED associated with the key will indicate a message to the extension.

Press the key to listen to the message. By pressing the key a call is made to the voice mail system. This command is used to define the number to be called, e.g. the number of the analogue extension connecting the voice mail system.

If the external voice mail system is connected via more than one extension line, a PBX-group should be created. The PBX-group should be programmed to contain all extension lines used to connect the voice mail system, and this command should specify the number of the PBX-group.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004