BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2002
Tone signal scheme

The tone signal scheme controls the frequency and cadence of each tone message.

0 = Standard (CCITT)

1 = Sweden

2 = Australia

3 = Finland

4 = Denmark

5 = Norway

6 = Belgium

7 = New Zealand

8 = New Zealand with disconnection tone

9 = Switzerland

10-99 Not defined (standard CCITT will be used)

Note

Normally the PABX shall also be equipped with a market-adapted EXU-board in order to obtain the correct tone frequencies and levels

Revision: G © Ericsson Enterprise 2004