BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2407
Digit for Radio paging

An extension that receives no answer on a call to a free extension can initiate paging by pressing a predetermined key.

Dependent on the type of receiver possessed by the pagee, either meet-me paging or “call-me” paging is started. See command group 81 for more information.

This command is used to determine the digit to be used for paging.

Only extensions with a service category permitting initiation of paging are allowed to initiate paging. See command 3064 Paging.

If the digit has been used previously for another facility, it will be erased for this facility, i.e. the “old” facility will be removed from the system. See the other commands in this command group.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004