BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8801
DISA error reroute position

When an external party connected to the facility “DISA with Password Control” (see command 5425 Create DISA with password) sends digits which do not correspond to an option in the current menu level, an error announcement will be played (see command 4423 DISA voice prompts).

If there is a second wrong response in the same menu level or resources are missing, the caller will be rerouted to the directory number stated in this command.

If no resource position is defined (DIR.NONUM), the call will be rerouted to the rewriting position of the incoming trunk (see commands 1103 Reroute position at day, 1104 Reroute position at night).

Possible EXIT-positions for DISA:

- OP-queue
- Operator
- Extension
- PBX
- ACD

##### Valid data

Decimal number |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004