BusinessPhone Communication Platform 6.0
Commands > Commands 6000...6999

## 6301
Log outgoing calls ?

The command is used to determine whether or not outgoing external calls are to be logged.

If it is desired to log outgoing external calls, but not all of them, it is possible to define more detailed which outgoing calls are to be logged. See commands 6302 Log duration time, 6303 Log minimum meter pulses and 6306 Log dialled numbers beginning with 0-6315 Log dialled numbers beginning with 9.

##### Valid data

Yes |  |  |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004