BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3505
PBX queue overflow time

This command defines, how long a call will be queued in a PBX queue. After this time has been elapsed, the call will be rerouted to the exit position of the PBX group.

##### Valid data

0 - 255 |  | (seconds) The value 0 will be interpreted as no queueing for the particular PBX group. A call, which arrives at a busy PBX group, will be rerouted immediately to the exit position of the PBX group. If no exit position has been defined, the default busy behaviour will take place. |
255 |  | (default) |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004