BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0109
Diversion active?

Direct diversion means that all incoming calls to the extension are diverted to a nominated answering address (diverted position).

Direct diversion is normally activated and deactivated by the extensions but this can also be made with this command.

For a diversion to take place, the extension must have been programmed, see command 0112 Destination of fixed diversion.

Only one of the facilities “direct diversion” or “follow-me” can be activated at the same time. If one facility is activated, the other will automatically be deactivated.

“Follow-me” and “direct diversion” can also be initiated and erased by extension users, with the DIVERSION key or by using *,# -procedures.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: 0

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004