BusinessPhone Communication Platform 6.0
Commands > Commands 7000...7999

## 7447
Heartbeat pace

This command determines the number of hours between two calls from the heartbeat function. Value 1-255 hours.

‘Heartbeat’ means that the PABX makes a call to a specified external number to show that it has not stopped functioning.

Commands 7420 Service area id, 7421 Identity of exchange and 7440 Heartbeat on?-7447 Heartbeat pace concern the heartbeat function.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004