BusinessPhone Communication Platform 6.0
Commands > Commands 6000...6999

## 6204
Digits to log

The dialled digits in case of call metering may differ from those sent if Least Cost Routing is used. With this command it can be defined which digits you want to have logged. This definition applies for all formats except the CIL2 format.

Set the command 6204 Digits to log to “YES” if you want to log the sent digits.

Set the command 6204 Digits to log to “NO” if you want to log the dialled digits.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004