BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8017
Wake-up order ref 3

A guest who orders a wake-up call from a telephone without display will receive a voice message as acknowledgement. This command defines the voice reference to be used.

The reference number is entered as : uuvv

where

uu = 01 (always) |  |

vv = 01-32 (see command 4401 Voice Announcements) |  |

uuvv = 0000 (no voice answer) |  |

It is required that the stated reference (uuvv) has been recorded with a system telephone in accordance with command 4401 Voice Announcements.

Wake-up acknowledgements can be supplied in three different languages.

With commands 8009 Wake-up language 1-8011 Wake-up language 3 the three languages in which wake-up-messages can be given are stated. Commands 8015 Wake-up order ref 1-8017 Wake-up order ref 3 are used to determine the wake-up acknowledgements to be supplied for the respective language.

This command is used to determine the wake-up acknowledgement to be supplied for the current language.

##### Valid data

Format: |  | iijj |
ii |  | {00,01} |
jj |  | {01-32} |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004