BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1802
Pre-digits at automatic incoming traffic

The command is used to state the digits that shall be inserted before the incoming number before it is analyzed.

Valid data: 1-2 digits

##### Valid data

1 |  | (digits) |
2 |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004