BusinessPhone Communication Platform 6.0
Commands > Commands 3000...3999

## 3504
PBX queue announcement delay

This command defines the time before the queue announcement will be played for a PBX group.

A valid value will range from 6 to 15 seconds.

It is supposed that a queue announcement has been defined and recorded.

(see commands 3503 PBX queue announcement reference and 4436).

##### Valid data

6-15 |  | (seconds) |

Default data: 6

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004