BusinessPhone Communication Platform 6.0
Commands > Commands 9000...9999

## 9111
NPI for private/public called number 1

The command is used to define the Number Plan Identifier (Number Plan and Type Of Number) of the called number.

Following combinations of NPI's are available for the private network (CN) calls:

value | Number Plan | Type Of Number
00h | Public | Unknown
01h | Public | International
02h | Public | National
04h | Public | Subscriber
10h (default) | Private | Unknown
12h | Private | Regional level 1
14h | Private | Regional level 0 (local)
20h | Unknown | Unknown *

- * Used e.g. when characters * and # are send as digit-information in a number

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004