BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0xC9
Invalid TEI Value

Default definition: |  | ERROR |
Used by block: |  | TR |
Category: |  | MAINTENANCE |

A call setup attempt was denied, because of an invalid terminal TEI value.

- D1: Card position
- D2: Individual number
- D3: Faulty TEI value
- D4: Undefined

#### Recommended action

Check the TEI value at the ISDN terminal and/or command 1957 ‘Assigned TEI Values’. Valid TEI values are programmed (0-63) or automatically assigned (64-126).

Revision: I © Ericsson Enterprise 2004