BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8112
Mode digit meet-me

Command 8103 Mode digit is used to determine whether a mode digit shall be sent to the paging equipment. ASB150 can only send single digit mode digits.

The mode digits that are sent to the paging equipment have a permanent functional significance that depends on the different paging units available in the various markets.

Commands 8112 Mode digit meet-me-8115 Mode digit group and 8118 Mode digit external call are used to determine the mode digits to be sent for the different forms of standard paging.

This command is used to determine the mode digit to be sent for an internal call that starts meet-me paging.

Range of values = 0-9

The function “internal meet-me call” can be removed from the system by writing over the mode digit with the space character.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004