BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0101
Facility COS

The facility category controls the number of facilities the extension has access to.

Extensions (and trunk lines) can be divided into 16 different facility categories.

##### Valid data

0 |  | (default) |
1-15 |  |  |

For each category and each facility, it is possible to determine whether it is permitted to use the facility or not. See command group 30.

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004