BusinessPhone Communication Platform 6.0
Commands > Commands 0000...0999

## 0701
Registration password

The command defines the password of an IP-Extension, being used for authentication purpose during the registration of an H.323 compliant IP-phone/IP-client at the gatekeeper. If the received password from the IP-phone/IP-client does not match to the one stored in ASB 150 02, the Gatekeeper will reject the registration and the IP-phone/IP-client will not be able to generate any traffic.

##### Valid data

20 characters |  | Only the defined password will be accepted |
empty (default) |  | Any password will be accepted |

Note

The Ericsson IP-phones Dialog 3413, 4422 and 4425 only support numeric characters

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: F © Ericsson Enterprise 2004