BusinessPhone Communication Platform 6.0
Warning Messages ASB 150 02 >

## 0x99
Warning Log Full

Default definition: |  | ALARM + INFO + NOPROG + EXTERN + ACTIVE |
Used by block: |  | OM |
Category: |  | MAINTENANCE |

This warning is used for the logs ERROR, ALARM and STOP. It is sent, when the number of free positions in the logarea becomes less or equal to the number specified by the constant OM.LOWALIM. The interpretation of the warning should be that the EEPROM logarea is becoming full. If this condition is allowed to continue, warning messages will be lost. Read the information in the logareas and reset the logs.

- D1:
- D2: Type of logarea

- 01h: ERROR logarea
- 02h: ALARM logarea
- 03h: STOP logarea

- D3: Undefined
- D4: Undefined

Revision: I © Ericsson Enterprise 2004