BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2403
Digit for Call pick up

If a user hears a call ringing at another extension, he/she may answer the call at his/her own extension by dialling the ringing extension’s number followed by a digit after the busy tone has been received.

This command determines the digit to be used for call pickup.

If the digit is already used for another service, it will be erased for this service, i.e. the “old” service is removed from the system. See other commands in this group.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004