BusinessPhone Communication Platform 6.0
Commands > Commands 5000...5999

## 5432
Create Private Network Access Code

In ASB 150 02, the private network router (PNR) is intended to be an own isolated routing mechanism, which will have the following main tasks:

- Routing based on dialled private network access code
- 3 alternative route selections in case of busy trunks
- Destination number conversion based on choosen route

This command will create a new private network access code (PNAC). The private network access code could be a network location code (LOC) or a co-ordinated numbering plan (CNP) directory number.

ASB 150 02 allows a maximum of 1000 private network access codes.

Note

Command 5532 Delete Private Network Access Code is used to delete the directory number for this facility.

Note

Command 5632 Change of Private Network Access Code is used to alter the directory number for this facility.

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004