BusinessPhone Communication Platform 6.0
Facilities

## Call Pick-Up – Individual

## Definition

The possibility to answer an internal or external ringing call from any telephone (extension).

## Use

Allows an extension user, from his own telephone, to pick up a call to a colleague's telephone.

## Operation

### All types of telephone

For a call to another telephone's directory number:

1. Dial directory number of the extension where the call is ringing.
2. On receipt of busy tone dial requisite postdialling digit (normally 6).

- Speech connection is established with caller.
- Ringing to original extension ceases.

#### DBC 223, DBC 213 and DBC 662 telephones

When you call a ringing extension, on depression of pick‑up the ringing call is picked up.

#### DBC 223, DBC 213, DBC 662, DBC 222, DBC 212 and DBC 631 telephones

After pick up the display shows:

The top row shows from whom the call was picked up.

The second row shows the connected party.

## Capacity

Not applicable.

## Limitations

Only calls that ring at the extension (Line 1 and Line 2) can be picked up.

On answer no authorisation check is made in the traffic group matrix.

This means that the user can pick up any call even those that are normally blocked and not through-connected.

To prevent this, the system has to be reprogrammed.

## Programming

2403 |  | Digit for Call pick up

If a user hears a call ringing at another extension, he may answer the call at his/her own extension by dialling the ringing extension's number followed by a digit after the busy tone has been received.

This command determines the digit to be used for call pickup.

## Equipment

None

Revision: C © Ericsson Enterprise 2004