BusinessPhone Communication Platform 6.0
Commands > Commands 8000...8999

## 8713
Automated Attendant error reroute position

In selections list it is possible to program an exit position (for time-out and cases of wrong entries).

In this command you must specify the directory number of the exit position.

##### Valid data

Decimal number |  |  |

Minimum required authority level from telephone: 1

Accessible via BMS: Yes

Revision: D © Ericsson Enterprise 2004