BusinessPhone Communication Platform 6.0
Commands > Commands 2000...2999

## 2613
Signal time

This command defines the tone time per digit for digit sending with DTMF.

Value: 0-65535

N.B! Tone time = 65535 means continuous tone sending (of first keyed digit). Intended for use when measuring the DTMF-signal. |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: G © Ericsson Enterprise 2004