BusinessPhone Communication Platform 6.0
Dialogs

## Swap Extensions

You can swap extensions of the same type. Swapping an extension means moving the extension data from one card or individual to another. When the physical connection of two extensions has been exchanged, both will still show their previously assigned data (directory number, parameters, keys, terminal type, etc.).

To access the dialog, open the “Extensions” menu in the Configuration directory view and click on one of the submenus. This will bring up the respective context menu. Select “Swap extensions” to open the dialog.

For further information, see also command:

5603 |  | Swap Extension (Change of line position for extension)

### View extension parameters

- To view the extension parameters, select a Directory Number from the drop-down list or enter the directory number in the field on the right side.
- Click on the “Go to extension” link. See section Extension Parameter.

### Swapping extensions

- Select the first extension from the drop-down list.
- Select the second extension.
- Click on the Submit button.

The dialog refreshes, now showing blank fields. If no error message was displayed, the extensions have been swapped successfully.

#### Actions

Submit |  | To send the settings to the system. |
Reload |  | To retrieve the settings from the system. |

Revision: B © Ericsson Enterprise 2004