BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1009
Reroute on answering position barred?

The command is to be used for in-dialing and for private lines to reroute calls to the rerouting position. Rerouting takes place if the call is made to a barred extension.

For rerouting to take place, the rerouting position must have been programmed, see commands 1103 Reroute position at day and 1104 Reroute position at night.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004