BusinessPhone Communication Platform 6.0
Commands > Commands 1000...1999

## 1718
Blocking on separate E2, M2 wires?

The command is used to state wheter blocking on separate wires (E2, M2) is to be used.

Note

Ascertain wheter the signal is included in the selected line signal scheme.

##### Valid data

Yes |  | (default) |
No |  |  |

Minimum required authority level from telephone: No

Accessible via BMS: Yes

Revision: E © Ericsson Enterprise 2004